{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":53,"n_cols":5,"rows_kept":53,"merged":[[0,0,0,4],[2,1,18,1],[19,1,24,1],[26,1,27,1],[26,4,27,4],[29,1,32,1],[29,4,32,4],[34,1,36,1],[38,1,43,1],[44,1,49,1],[52,1,52,4]]}
["室外台阶及地面石材铺贴工程量汇总表（㎡）"]
["序号","楼号","计算式","工程量","备注"]
[1,"教学楼一","3.2*1.6",{"$f":"3.2*1.6","v":{"v":5.120000000000001,"d":"5.12"}}]
[2,null,"0.14*(1.6+1.6+3.2+1.3+1.3+2.6+1+1+2) ",{"$f":"0.14*(1.6+1.6+3.2+1.3+1.3+2.6+1+1+2)","v":{"v":2.184,"d":"2.18"}}]
[3,null,"3.8*2.1",{"$f":"3.8*2.1","v":{"v":7.9799999999999995,"d":"7.98"}}]
[4,null,"0.14*(2.1+2.1+3.8+1.8+1.8+3.2+1.5+1.5+2.6)",{"$f":"0.14*(2.1+2.1+3.8+1.8+1.8+3.2+1.5+1.5+2.6)","v":{"v":2.8560000000000008,"d":"2.86"}}]
[5,null,"2.6*1.6",{"$f":"2.6*1.6","v":4.16}]
[6,null,"0.14*(3.2+1.6+1.6+1.3+1.3+2.6+2+1+1)",{"$f":"0.14*(3.2+1.6+1.6+1.3+1.3+2.6+2+1+1)","v":{"v":2.184,"d":"2.18"}}]
[7,null,"3.8*1",{"$f":"3.8*1","v":{"v":3.8,"d":"3.80"}},"未破损"]
[8,null,"0.14*(3.8+1+1+3.2+0.7+0.7+2.6+0.4+0.4)",{"$f":"0.14*(3.8+1+1+3.2+0.7+0.7+2.6+0.4+0.4)","v":{"v":1.932,"d":"1.93"}}]
[9,null,"3.2*1.6",{"$f":"3.2*1.6","v":{"v":5.120000000000001,"d":"5.12"}}]
[10,null,"0.14*(3.2+1.6+1.6+2.6+1.3+1.3+2+1+1)",{"$f":"0.14*(3.2+1.6+1.6+2.6+1.3+1.3+2+1+1)","v":{"v":2.1840000000000006,"d":"2.18"}}]
[11,null,"5.4*2.7",{"$f":"5.4*2.7","v":{"v":14.580000000000002,"d":"14.58"}}]
[12,null,"0.14*(5.4+5.4+4.8+4.2+2.4+2.2+1.9+2.8+0.5)",{"$f":"0.14*(5.4+5.4+4.8+4.2+2.4+2.2+1.9+2.8+0.5)","v":{"v":4.144,"d":"4.14"}}]
[13,null,"5.5*2.4",{"$f":"5.5*2.4","v":{"v":13.2,"d":"13.20"}}]
[14,null,"0.14*(8+7+6+1.5)",{"$f":"0.14*(8+7+6+1.5)","v":{"v":3.1500000000000004,"d":"3.15"}}]
[15,null,"5.5*2.4",{"$f":"5.5*2.4","v":{"v":13.2,"d":"13.20"}}]
[16,null,"0.14*(8+7+6+1.5)",{"$f":"0.14*(8+7+6+1.5)","v":{"v":3.1500000000000004,"d":"3.15"}}]
["小计",null,null,{"$f":"SUM(D3:D18)","v":{"v":88.944,"d":"88.94"}}]
[17,"体育馆","4.7*2.5+0.14*（4.4+4.7+4.7）",{"$f":"4.7*2.5+0.14*(4.4+4.7+4.7)","v":{"v":13.682,"d":"13.68"}}]
[18,null,"6.3*1.2+0.14*（1.2+1.2+1.2）",{"$f":"6.3*1.2+0.14*(1.2+1.2+1.2)","v":{"v":8.064,"d":"8.06"}}]
[19,null,"1.5*5.8",{"$f":"1.5*5.8","v":{"v":8.7,"d":"8.70"}}]
[20,null,"0.1*（5.8+5.8+4.3+4.3+2.3+2.3）",{"$f":"0.1*(5.8+5.8+4.3+4.3+2.3+2.3)","v":{"v":2.4800000000000004,"d":"2.48"}}]
[21,null,"3.5*1",{"$f":"3.5*1","v":{"v":3.5,"d":"3.50"}}]
[22,null,"5.3*2.4+0.14*（5.8+5.8）",{"$f":"5.3*2.4+0.14*(5.8+5.8)","v":{"v":14.344,"d":"14.34"}}]
["小计",null,null,{"$f":"SUM(D20:D25)","v":50.77}]
[23,"英语楼","2.2*1.6",{"$f":"2.2*1.6","v":{"v":3.5200000000000005,"d":"3.52"}},"其他部位未破损"]
[24,null,"0.14*(2.2+2.2+2.2)",{"$f":"0.14*(2.2+2.2+2.2)","v":{"v":0.9240000000000002,"d":"0.92"}}]
["小计",null,null,{"$f":"SUM(D27:D28)","v":{"v":4.444000000000001,"d":"4.44"}}]
[25,"中文楼","3.6*1+0.14*（3.6+3.6）",{"$f":"3.6*1+0.14*(3.6+3.6)","v":{"v":4.6080000000000005,"d":"4.61"}},"其他部位未破损"]
[26,null,"5.4*3.6",{"$f":"5.4*3.6","v":19.44}]
[27,null,"4.8*1.2",{"$f":"4.8*1.2","v":5.76}]
[28,null,"0.1*（4.8+4+2.8+2+0.45）",{"$f":"0.1*(4.8+4+2.8+2+0.45)","v":{"v":1.4050000000000002,"d":"1.41"}}]
["小计",null,null,{"$f":"SUM(D30:D33)","v":{"v":31.213,"d":"31.21"}}]
[29,"食堂","11.7*2.7+0.14*（11.7+11.7+11.7）",{"$f":"11.7*2.7+0.14*(11.7+11.7+11.7)","v":{"v":36.504,"d":"36.50"}}]
[30,null,"7.3*2.7+0.14*（7.3+7.3+7.3）",{"$f":"7.3*2.7+0.14*(7.3+7.3+7.3)","v":{"v":22.776,"d":"22.78"}}]
[31,null,"2*1.4+0.14*（2+2+2）",{"$f":"2*1.4+0.14*(2+2+2)","v":{"v":3.6399999999999997,"d":"3.64"}}]
["小计",null,null,{"$f":"SUM(D35:D37)","v":62.92}]
[32,"行政楼","3.4*2.3",{"$f":"3.4*2.3","v":{"v":7.819999999999999,"d":"7.82"}}]
[33,null,"0.14*（1.1+1.1+2.2+1.5+1.5+2.8+2+2+3.4+3.4）",{"$f":"0.14*(1.1+1.1+2.2+1.5+1.5+2.8+2+2+3.4+3.4)","v":2.94}]
[34,null,"6.7*2.4",{"$f":"6.7*2.4","v":16.08}]
[35,null,"0.14*（8+9.1+0.5+8）",{"$f":"0.14*(8+9.1+0.5+8)","v":{"v":3.5840000000000005,"d":"3.58"}}]
[36,null,"4*2+0.14*（6+5.4+4.8）",{"$f":"4*2+0.14*(6+5.4+4.8)","v":{"v":10.268,"d":"10.27"}}]
["小计",null,null,{"$f":"SUM(D39:D43)","v":{"v":40.69199999999999,"d":"40.69"}}]
[37,"招生楼","3.4*2",{"$f":"3.4*2","v":{"v":6.8,"d":"6.80"}}]
[38,null,"0.14*（1.7+1.7+3.4+3.4+2.8+1.4+1.4+2.2+1.1+1.1）",{"$f":"0.14*(1.7+1.7+3.4+3.4+2.8+1.4+1.4+2.2+1.1+1.1)","v":{"v":2.8280000000000007,"d":"2.83"}}]
[39,null,"3.2*1.8",{"$f":"3.2*1.8","v":{"v":5.760000000000001,"d":"5.76"}}]
[40,null,"0.14*（3.2+1.8+2.9+2.6+1.5+1.2）",{"$f":"0.14*(3.2+1.8+2.9+2.6+1.5+1.2)","v":{"v":1.848,"d":"1.85"}}]
[41,null,"5.3*2.4",{"$f":"5.3*2.4","v":{"v":12.719999999999999,"d":"12.72"}}]
[42,null,"0.14*（8+0.9+0.7+0.3+2.1+1.8+5.2+4.6）",{"$f":"0.14*(8+0.9+0.7+0.3+2.1+1.8+5.2+4.6)","v":{"v":3.3040000000000007,"d":"3.30"}}]
["小计",null,null,{"$f":"SUM(D45:D50)","v":33.26}]
[43,"场地","5.2*4",{"$f":"5.2*4","v":{"v":20.8,"d":"20.80"}}]
["总计",{"$f":"D19+D26+D29+D34+D38+D44+D51+D52+2.96","v":{"v":336.003,"d":"336.00"}}]

{"sheet":"Sheet2","index":1,"n_rows":70,"n_cols":4,"rows_kept":70,"merged":[[0,0,1,3],[3,0,7,0],[9,0,12,0],[14,0,19,0],[20,0,23,0],[28,0,29,3],[69,0,70,3]]}
["上海韩国学校外籍人员子女学校室外台阶石材铺贴、栏杆更换工程"]
[]
["项目名称","序号","细节","备注"]
["火烧面花岗岩更换",1,"原石材拆除","原始石材拆除，短驳至校方指定位置"]
[null,2,"拆除垃圾外运","使用环卫车将建筑垃圾外运出场"]
[null,3,"细石砼基础找平","使用自拌细石混凝土对基础找平"]
[null,4,"踏步面石材铺贴","海螺P.C 42.5水泥干铺，粗纱，火烧面花岗岩,厚度30mm"]
[null,5,"侧石石材铺贴","火烧面花岗岩,厚度20mm"]
[null,6,"磨边及防滑","切割及磨小圆边"]
["无障碍通道扶手更换",1,"原扶手拆除","原不锈钢扶手拆除，包含基础预埋件及周围石材一起拆除"]
[null,2,"扶手埋板制作安装","制作100*100*2mm预埋钢板"]
[null,3,"不锈钢扶手制作安装","SUS 304不锈钢、大管5.1cm、厚度2.0毫米 、圆管"]
[null,4,"石材修复","海螺P.C 42.5水泥干铺，火烧面花岗岩,厚度30mm"]
[null,5,"扶手基础侧墙粉刷","室外防水涂料"]
["新建无障碍通道",1,"基础挖土并夯实","使用人工对素土地面开挖至老土，并堆放至校方指定位置"]
[null,2,"渣土垃圾外运","使用环卫车将建筑垃圾外运出场"]
[null,3,"混凝土地坪浇筑","商品混凝土C30浇筑基础"]
[null,4,"石材铺贴","海螺P.C 42.5水泥干铺，火烧面花岗岩,厚度30mm"]
[null,5,"扶手基础制作","C30混凝土浇筑扶手基础"]
[null,6,"不锈钢扶手制作安装","SUS 304不锈钢、大管5.1cm、厚度2.0毫米 、圆管"]
["食堂楼梯踏步更换",1,"石材拆除","原始石材拆除，短驳至校方指定位置"]
[null,2,"垃圾外运","使用环卫车将建筑垃圾外运出场"]
[null,3,"砂浆找平","使用自拌砂浆对基础找平"]
[null,4,"踏步石材铺贴","海螺P.C 42.5水泥干铺，抛光大理石,厚度30mm，长度1750,通铺"]
["教学楼至食堂地面修补",1,"踏步石材铺贴","海螺P.C 42.5水泥干铺，火烧面花岗岩,厚度30mm"]
["教学楼一层走廊地面瓷砖修复",1,"地面找平瓷砖修复","瓷砖大小参考现有规格"]
[]
[]
["学校各栋楼出入口位置示意图"]
{"$rows_empty":40}
["台阶现状照片"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}